Clock Transition V2.1 Engineering Change Order (ECO)

1. Schematic pages 2-10

Remove RC filters for N+Guard

 Remove: C15, C30, C45, C60, C75, C90, C105, C120, C135

Remove: R15, R30, R45, R60, R75, R90, R105, R120, R135

1. Schematic page 11

Do NOT install jumpers at R194 and R195

Do Not Install Jumpers R188, R189, R190 and R191

1. Schematic pages 2-10

Modify RC filters for waveshaping on vertical clocks

 Change to 0.1uF: C11, C12, C13

 C26, C27, C28

 C41, C42, C43

 C56, C57, C58

 C71, C72, C73

 C86, C87, C88

 C101, C102, C103

 C116, C117, C118

 C131, C132, C133

 Change to 5 ohms: R11, R12, R13

 R26, R27, R28

 R41, R42, R43

 R56, R57, R58

 R71, R72, R73

 R86, R87, R88

 R101, R102, R103

 R116, R117, R118

 R131, R132, R133