Clock Transition V2.1 Engineering Change Order (ECO)

1. Schematic pages 2-10

Remove RC filters for N+Guard

Remove: C15, C30, C45, C60, C75, C90, C105, C120, C135

Remove: R15, R30, R45, R60, R75, R90, R105, R120, R135

1. Schematic page 11

Do NOT install jumpers at R194 and R195

Do Not Install Jumpers R188, R189, R190 and R191

1. Schematic pages 2-10

Modify RC filters for waveshaping on vertical clocks

Change to 0.1uF: C11, C12, C13

C26, C27, C28

C41, C42, C43

C56, C57, C58

C71, C72, C73

C86, C87, C88

C101, C102, C103

C116, C117, C118

C131, C132, C133

Change to 5 ohms: R11, R12, R13

R26, R27, R28

R41, R42, R43

R56, R57, R58

R71, R72, R73

R86, R87, R88

R101, R102, R103

R116, R117, R118

R131, R132, R133